;Register definition for LPC2100
;===============================
;
; name: user defined name of the register
; type: the type of the register
;	GPR	general purpose register
;	MM	memory mapped register
;	DMMx	direct memory mapped register with offset
;		x = 1..4
;		the base is defined in the configuration file
;		e.g. DMM1 0x02200000
; addr:	the number, adddress or offset of the register
; size	the size of the register (8,16 or 32)
;
;name		type	addr		size
;-------------------------------------------
;
sp		GPR	13
lr		GPR	14
pc		GPR	15
;
; User watchpoint register
;
wav0		ICEB    100
wam0		ICEB    101
wdv0		ICEB    102
wdm0		ICEB    103
wcv0		ICEB    104
wcm0		ICEB    105
;
wav1		ICEB    110
wam1		ICEB    111
wdv1		ICEB    112
wdm1		ICEB    113
wcv1		ICEB    114
wcm1		ICEB    115
;
; Watchdog
;
wdmod   	MM	0xE0000000	8
wdtc    	MM	0xE0000004	32
wdtv    	MM	0xE000000C	32
;
; System Control Block
;
extint  	MM	0xE01FC140	8
extwake 	MM	0xE01FC144	8
memmap  	MM	0xE01FC040	8
pllcon  	MM	0xE01FC080	8
pllcfg  	MM	0xE01FC084	8
pllstat 	MM	0xE01FC088	16
pllfeed 	MM	0xE01FC08C	8
pcon    	MM	0xE01FC0C0	8
pconp   	MM	0xE01FC0C4	32
vpbdiv  	MM	0xE01FC100	8
;

