;Register definition for MCF5235
;===============================
;
; name: user defined name of the register
; type: the type of the register
;	DREG	data register
;	AREG	address register
;	CREG	control register
;	MM	memory mapped register
;	DMMx	direct memory mapped register with offset
;		x = 1..4
;		the base is defined in the configuration file
;		e.g. DMM1 0x02200000
; addr:	the number, adddress or offset of the register
; size	the size of the register (8,16 or 32)
;
;name		type	addr		size
;-------------------------------------------
;
; Additional Control Register
;
other_a7        CREG    0x800           32
macsr           CREG    0x804           8
mask            CREG    0x805           16
acc0            CREG    0x806           16
accext01        CREG    0x807           16
accext23        CREG    0x808           16
acc1            CREG    0x809           16
acc2            CREG    0x80a           16
acc3            CREG    0x80b           16
flashbar        CREG    0xc04           32
rambar          CREG    0xc05           32
;
;
;
; DMM1 must be set to the internal memory base address
;
;       SDRAMC Registers
dcr             DMM1	0x040		16
dacr0           DMM1	0x048		32
dmr0            DMM1	0x04C		32
dacr1           DMM1	0x050		32
dmr1            DMM1	0x054		32
;
;       Chip Select Registers
csar0           DMM1	0x080		16
csmr0           DMM1	0x084		32
cscr0           DMM1	0x08A		16
csar1           DMM1	0x08C		16
csmr1           DMM1	0x090		32
cscr1           DMM1	0x096		16
csar2           DMM1	0x098		16
csmr2           DMM1	0x09C		32
cscr2           DMM1	0x0A2		16
csar3           DMM1	0x0A4		16
csmr3           DMM1	0x0A8		32
cscr3           DMM1	0x0AE		16
csar4           DMM1	0x0B0		16
csmr4           DMM1	0x0B4		32
cscr4           DMM1	0x0BA		16
csar5           DMM1	0x0BC		16
csmr5           DMM1	0x0C0		32
cscr5           DMM1	0x0C6		16
csar6           DMM1	0x0C8		16
csmr6           DMM1	0x0CC		32
cscr6           DMM1	0x0D2		16
;
;       Watchdog Timer Registers
wcr             DMM1	0x140000	16
wmr             DMM1	0x140002	16
wcntr           DMM1	0x140004	16
wsr             DMM1	0x140006	16


