;Register definition for Feroceon 966 (Dragonite)
;================================================
;
; name: user defined name of the register
; type: the type of the register
;	GPR	general purpose register
;	CP15	CP15 register
;	MM	memory mapped register
;	DMMx	direct memory mapped register with offset
;		x = 1..4
;		the base is defined in the configuration file
;		e.g. DMM1 0x02200000
; addr:	the number, adddress or offset of the register
; size	the size of the register (8,16 or 32)
;
;name		type	addr		size
;-------------------------------------------
;
;
; CP15 Registers
;
;  Register Numbers for Fero966:
;  +-------+-------+-------+-------+
;  | | | | | | | | | | | | | | | | |
;  +-+-----+-+-----+-------+-------+
;  |-|opc_1|-|opc_2|  CRm  |  nbr  |
;  +-+-----+-+-----+-------+-------+
;
;
id		CP15    0x0000          32      ;ID code
control 	CP15    0x0001          32      ;Control
;


