;Register definition for AT91SAM7S
;=================================
;
; name: user defined name of the register
; type: the type of the register
;	GPR	general purpose register
;	MM	memory mapped register
;	DMMx	direct memory mapped register with offset
;		x = 1..4
;		the base is defined in the configuration file
;		e.g. DMM1 0x02200000
; addr:	the number, adddress or offset of the register
; size	the size of the register (8,16 or 32)
;
;name		type	addr		size
;-------------------------------------------
;
sp		GPR	13
lr		GPR	14
pc		GPR	15
;
;
; Embedded Flash Controller
;
mc_fmr  	MM	0xFFFFFF60	32
mc_fcr  	MM	0xFFFFFF64	32
mc_fsr  	MM	0xFFFFFF68	32
;
; Watchdog Timer
;
wdt_cr  	MM	0xFFFFFD40	32
wdt_mr  	MM	0xFFFFFD44	32
wdt_sr  	MM	0xFFFFFD48	32
;
; Reset Controller
;
rstc_cr 	MM	0xFFFFFD00	32
rstc_sr 	MM	0xFFFFFD04	32
rstc_mr 	MM	0xFFFFFD08	32
;
; Power Management Controller
;
pmc_scer	MM	0xFFFFFC00	32
pmc_scdr	MM	0xFFFFFC04	32
pmc_scsr	MM	0xFFFFFC08	32
pmc_pcer	MM	0xFFFFFC10	32
pmc_pcdr	MM	0xFFFFFC14	32
pmc_pcsr	MM	0xFFFFFC18      32
ckgr_mor	MM	0xFFFFFC20	32
ckgr_mcfr       MM	0xFFFFFC24	32
ckgr_pllr       MM	0xFFFFFC2C	32
pmc_mckr	MM	0xFFFFFC30	32
pmc_pck0	MM	0xFFFFFC40	32
pmc_pck1	MM	0xFFFFFC44	32
pmc_ier 	MM	0xFFFFFC60	32
pmc_idr 	MM	0xFFFFFC64	32
pmc_sr          MM	0xFFFFFC68	32
pmc_imr 	MM	0xFFFFFC6C	32






