;Register definition for ARM7
;============================
;
; name: user defined name of the register
; type: the type of the register
;	GPR	general purpose register
;	MM	memory mapped register
;	DMMx	direct memory mapped register with offset
;		x = 1..4
;		the base is defined in the configuration file
;		e.g. DMM1 0x02200000
; addr:	the number, adddress or offset of the register
; size	the size of the register (8,16 or 32)
;
;name		type	addr		size
;-------------------------------------------
;
sp		GPR	13
lr		GPR	14
pc		GPR	15
;



