;Register definition for IQ80310
;===============================
;
; name: user defined name of the register
; type: the type of the register
;	GPR	general purpose register
;	CP15	CP15 register
;	MM	memory mapped register
;	DMMx	direct memory mapped register with offset
;		x = 1..4
;		the base is defined in the configuration file
;		e.g. DMM1 0x02200000
; addr:	the number, adddress or offset of the register
; size	the size of the register (8,16 or 32)
;
;
; CP15 Registers Numbers for xScale:
;
;       +-----+-+-------+-----+-+-------+
;       |opc_2|0|  CRm  |opc_1|0|  nbr  |
;       +-----+-+-------+-----+-+-------+
;
; The 16bit register number is used to build the appropriate MCR/MRC instruction.
;
;
;name		type	addr		size
;-------------------------------------------
;
id		CP15    0x0000          32      ;ID code
cache   	CP15    0x2000          32      ;Cache type
ctr             CP15    0x0001          32      ;Control
aux     	CP15    0x2001          32      ;Auxiliary Control
ttb             CP15    0x0002          32      ;Translation Table Base
dac             CP15    0x0003          32      ;Domain Access Control
fsr     	CP15    0x0005          32      ;Fault Status
far     	CP15    0x0006          32      ;Fault Address
pid        	CP15    0x000d          32      ;Process ID
cpacc      	CP15    0x010f          32      ;Coprocessor Access
;
;
;       80312 Memory controller
;
sdir            MM      0x00001500
sdcr            MM      0x00001504
sdbr            MM      0x00001508
sbr0            MM      0x0000150c
sbr1            MM      0x00001510
;
eccr            MM      0x00001534
elog0           MM      0x00001538
elog1           MM      0x0000153c
ecar0           MM      0x00001540
ecar1           MM      0x00001544
ectst           MM      0x00001548
febr0           MM      0x0000154c
febr1           MM      0x00001550
fbsr0           MM      0x00001554
fbsr1           MM      0x00001558
fwsr0           MM      0x0000155c
fwsr1           MM      0x00001560
mcisr           MM      0x00001564
rfr             MM      0x00001568

